|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| \*Por favor, llene las siguientes Casillas del rating del avión/ Please, fill out the following box for Aircraft Ratings | | | | Por favor, llene las siguientes Casillas para los demás Ratings/Please, fill out the following box for other Ratings | | | | | | | | |
| **Aircraft Type and Model/**  **Tipo y Modelo de Aeronave:** | N/A | | | **Component P/N/**  **P/N del componente:** | | | All Part Numbers listed in Operating and Maintenance Manual (OMM) 24-30-99 | | | | | |
| **Aircraft Manufacturer/**  **Fabricante de la aeronave:** | N/A | | | **Component Name/**  **Nombre del componente:** | | | BATTERY | | | | | |
| **Manufacturer Maintenance Manual/**  **Manual de Mantenimiento del Fabricante** | **Description/**  **Descripción** | **Revision/**  **Revisión** | **Date/**  **Fecha** | **Component Manufacturer/**  **Fabricante del componente:** | | | SAFT | | | | | |
| N/A | N/A | N/A | **Manufacturer Maintenance Manual/**  **Manual de mantenimiento del Fabricante** | | | **Description/**  **Descripción** | | **Revision/**  **Revisión** | | **Date/**  **Fecha** | |
| 24-30-99 | | REV 30 | | 14-FEB-2024 | |
| **Scope/**  **Alcance** | OVH | REP | | INSP | TEST | CHECK | | OTHER |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Item/** | **Task Number/ Número de la Tarea** | **Threshold / Interval /** | **Tools and Equipment /** | **P/N or Ref. /** | **Equivalent P/N/ P/N Equivalente** | **Qty. /** | **Comments /** |
| **Ítem** | **Umbral/Intervalo** | **Herramienta y equipo** | **P/N o Referencia** | **Cantidad** | **Comentarios** |
| 1 | - | General Overhaul | Constant current charger (DC current range 0-60A, minimum open DC voltage 40V | Local supplier | - | 1 | - |
| 2 | - | General Overhaul | Special tool kit | 416161 | - | 1 | - |
| 3 | - | General Overhaul | Constant current load Bank (DC current range 0-60 A, DC voltage range 1-40V | Local supplier | - | 1 | - |
| 4 | - | General Overhaul | Megohmmeter (0-50MΩ @ 250VDC) | Local supplier | - | 1 | - |
| 5 | - | General Overhaul | Multimeter (Volt, Ω,mA) 3.5 digits 2000 counts 1% or better | Local supplier | - | 1 | - |
| 6 | - | General Overhaul | Climatic chamber or temperatura control device | Local supplier | Proskit Soldering and Desoldering Station P/N SS-989E and Multimeter | 1 | Required only If battery has a sensor |
| 7 | - | General Overhaul | Torque wrench 0-15N.m (0-133 lbf.in) | Local supplier | - | 1 | - |
| 8 | - | General Overhaul | Standard mechanic´s tools | Local supplier | - | 1 | - |
| 9 | - | General Overhaul | Stiff bristle brush (non-metallic) | Local supplier | - | 1 | - |
| 10 | - | General Overhaul | Small paintbrush (non-metallic) | Local supplier | - | 1 | - |
| 11 | - | General Overhaul | Dry, compressed air source (Less than 1.4 bar (20 psi)) | Local supplier | - | 1 | - |
| 12 | - | General Overhaul | Soft, lint free, clean cloth | Local supplier | - | 2 | - |
| 13 | - | - | - | - | - | - | - |
| 14 | - | - | - | - | - | - | - |
| 15 | - | - | - | - | - | - | - |